**Building Consenting Unit**

**Construction Statement –**

**solid/liquid fuel heater**

|  |
| --- |
| **This statement must be completed by the installer and be provided to the building inspector at the time of the inspection.** |

**TO: Christchurch City Council Building Consent Authority**

**Issued by:** *(name of installer)*

|  |
| --- |
|  |

In respect of building consent number: At: *(project address)*

|  |  |
| --- | --- |
|  |  |

In relation to the installation of a:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| solid fuel heater | liquid fuel heater | free-standing | in-built | insert |

Make: Model:Serial No:

|  |  |  |
| --- | --- | --- |
|  |  |  |

| *[Select as appropriate]* | **Yes** | **No** | **N/A** |
| --- | --- | --- | --- |
| The existing chimney has been cleaned and inspected for soundness prior to installation. |  |  |  |
| The fireplace surround / chimney face junction is sealed up with heat resistance material. |  |  |  |
| The flue pipe is constructed of austenitic stainless steel. |  |  |  |
| Seismic restraint has been fitted. |  |  |  |
| The flue sections are secured together with stainless steel rivets. |  |  |  |
| The flue is secured to the appliance. |  |  |  |
| Flue/enclosure has been vented. |  |  |  |
| Flue and appliance clearances have been achieved in terms of the manufacturer’s installation instructions and AS/NZS 2918. |  |  |  |
| The flue height meets the minimum specified in the manufacturer’s instructions and Environment Canterbury (ECan) rules. |  |  |  |
| Flue flashing has been installed as specified in the manufacturer’s installation instructions. |  |  |  |
| The roofing underlay has been installed/repaired around flue penetration. |  |  |  |
| Smoke detectors (with hush facility) as detailed on the building consent documents are installed. |  |  |  |
| Connection or re- connection of wetback undertaken by Certifying Plumber, and details of this provided on form B-011 (Application for a code compliance certificate).  *Note: It is an offence under the Plumbers, Drainlayers and Gasfitters Act 2006 for unlicensed and unqualified persons to undertake this work.* |  |  |  |
| For **NEW** wetback connections, anti-scald device installed and copy of B-084 (Construction Statement – Pipework Testing) attached, completed and signed by the Certifying Plumber. |  |  |  |
| Liquid Fuel only:  The appliance has been installed and commissioned in accordance with the manufacturer’s installation and operating instructions, a copy of commissioning certificate is attached. |  |  |  |
| The liquid fuel storage tank and feed system has been installed in accordance with AS1691, or equivalent, and with the requirements of the Council’s Environmental Health Officer. |  |  |  |
| The fuel storage tank has secondary containment (100% if roofed, 120% if unroofed) in accordance with the proposed City Plan.  *Note: Audit monitoring will be carried out.* |  |  |  |

If response to any of the items is no, please comment:

|  |
| --- |
|  |

I (*print name)* certify that the above specified installation has been carried out as described and in accordance with the manufacturer’s installation instructions and the current approved building code requirements.

Installer’s Signature: Date:Registration No:

|  |  |  |
| --- | --- | --- |
|  |  |  |

I also understand that the Christchurch City Council, in accepting this construction statement, may be relying on it to issue the code compliance certificate at the completion of the building work.