**SITE ENTRY REQUIREMENTS**

**It is a Christchurch Waste Water Treatment Plant (CWTP) requirement that;**

* All Visitors must have an appointment and be accompanied by a CWTP employee whilst on site
* All Visitors and Contractors must sign in on arrival and out when leaving

**CONTRACTORS**

* All persons performing work at the CWTP are required to undergo a site induction
* You must adhere to the requirements of the Permit to Work system
* You follow all site rules / instructions
* Be aware of CWTP hazards and advise CWTP of any hazards you may introduce

******Minimum Personal Protective Equipment (PPE)** requirements in process areas: Hi-viz (day/night), safety footwear, eye protection, hard hat, and gloves.

**SITE HAZARDS**

* **Hazardous Areas and Atmospheres** (areas containing concentrations of flammable gases, vapours or dust) and oxygen deficient zones are present throughout the site.
* **Chemicals**-There are a mixture of acids, gases and other hazardous substances on site. Refer to Material Safety Data Sheets (MSDS)
* **Biological Hazards** –Hepatitis, Typhoid, Tetanus
* **Biogases –** Methane and Hydrogen Sulphide
* **Confined Spaces**
* **Mobile Plant / Equipment**– Loaders, Trucks, Cranes, etc.
* **Open Tanks and Ponds -**Aerated tanks with low buoyancy
* **Dynamic Hazards** – Refer to Dynamic Hazard Board and site map for temporary hazards, locations, and control methods.
* **Site Hazard Register** -Contact your site host to review the site hazard register

All **incidents / accidents** must be reported immediately to your CWTP host and an incident / accident form completed.